|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Index | File name | Number | Acrylic plates | Notes |
| A | A\_armWall\_waterTube | 4 | 5mm white | Contact with B or D boards |
| B | B\_armWall | 8 | 5mm white | Fixed on F (F1), and contact with A |
| C | A\_armWall\_waterTube | 1 |  |  |
| D1 | D1\_homeWall | 1 | 5mm white | Fixed on F (F1), and contact with A. |
| D2 | D2\_homeWallR | 1 | 5mm white | Fixed on F (F1), and contact with A. |
| E | E\_rotatorPlate | 1 | 5mm white | Rotatory plate, embedded in the center of F. |
| F1 | F1\_floor\_top\_asymmetry | 1 | 3mm white | Upper layer of floor, fixed with F2 |
| F2 | F2\_floor\_bottom\_asymmetry | 1 | 3mm white | Lower payer of floor, fixed with F2 |
| G | G\_foot | 5 | 10mm color un-limited | Bases, fixed under F (F2) |
| I | I\_homeDoorR | 6 | 3mm white | Cut and bend |
| J | J\_homeDoorL | 2 | 3mm white | Cut and bend |
| L | L\_Lid | 1 | 5mm transparent | Cut |